;
;   TivaWare data logger device driver installation file.
;
[Version]
Signature="$Windows NT$"
Class=Ports
ClassGuid={4D36E978-E325-11CE-BFC1-08002BE10318}
Provider=%MFGNAME%
LayoutFile=layout.inf
CatalogFile.NTx86=usb_dev_logger_x86.cat
CatalogFile.NTamd64=usb_dev_logger_amd64.cat
DriverVer=02/07/2014,2.1.0.12573

[Manufacturer]
%MFGNAME%=VirComDevice,NT,NTamd64

[DestinationDirs]
DefaultDestDir = 12

[VirComDevice.NT]
%DESCRIPTION%=DriverInstall,USB\Vid_1CBE&Pid_000b

[VirComDevice.NTamd64]
%DESCRIPTION%=DriverInstall,USB\Vid_1CBE&Pid_000b

[DriverInstall.NT]
Include=mdmcpq.inf
CopyFiles=FakeModemCopyFileSection
AddReg=DriverInstall.NT.AddReg

[DriverInstall.NT.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,usbser.sys
HKR,,EnumPropPages32,,"MsPorts.dll,SerialPortPropPageProvider"

[DriverInstall.NT.Services]
AddService=usbser, 0x00000002, DriverServiceInst

[DriverServiceInst]
DisplayName=%SERVICE%
ServiceType=1
StartType=3
ErrorControl=1
ServiceBinary=%12%\usbser.sys

[Strings]
MFGNAME     = "Texas Instruments, Inc."
DESCRIPTION = "TivaWare Data Logger Serial Port"
SERVICE     = "TivaWare USB CDC Serial Port"
