DOWNLOAD "Set Year.BAS"
REM *****SetYear Parameter to RTC*****
YEAR=05
EOP
SetYear
DOWNLOAD "DEMO.BAS"
SIZE 3,3
GAP 0,0
DENSITY 8
SPEED 4
DIRECTION 0
REFERENCE 0,0
SET CUTTER OFF
SET PEEL OFF
CLS
REM *****Read YEAR parameter form RTC*****
YEAR$=STR$(YEAR)
Y=YEAR
REM *****Print*****
TEXT 10,10,"5",0,1,1,"YEAR1="+YEAR$
TEXT 10,110,"5",0,1,1,"YEAR2="+STR$(Y)
TEXT 10,210,"5",0,1,1,"YEAR3="+STR$(YEAR)
PRINT 1
EOP
RUN "DEMO.BAS"
